libfc: recognize incoming FLOGI for point-to-point mode

When receiving a FLOGI request from a point-to-point peer,
the D_ID of 0xfffffe was not recognized as belonging to one
of the lports, so it was dropped.

Change fc_vport_id_lookup() to treat d_id 0xfffffe as a match.

Signed-off-by: Joe Eykholt <jeykholt@cisco.com>

---
 drivers/scsi/libfc/fc_npiv.c |    3 +++
 1 files changed, 3 insertions(+), 0 deletions(-)


---
diff --git a/drivers/scsi/libfc/fc_npiv.c b/drivers/scsi/libfc/fc_npiv.c
index c68f6c7..45b6f1e 100644
--- a/drivers/scsi/libfc/fc_npiv.c
+++ b/drivers/scsi/libfc/fc_npiv.c
@@ -72,6 +72,9 @@ struct fc_lport *fc_vport_id_lookup(struct fc_lport *n_port, u32 port_id)
 	if (fc_host_port_id(n_port->host) == port_id)
 		return n_port;
 
+	if (port_id == FC_FID_FLOGI)
+		return n_port;		/* for point-to-point */
+
 	mutex_lock(&n_port->lp_mutex);
 	list_for_each_entry(vn_port, &n_port->vports, list) {
 		if (fc_host_port_id(vn_port->host) == port_id) {
