fcoe: call fcoe_ctlr_els_send even for ELS responses

In point-to-point mode, the destination MAC address for
the FLOGI response was zero because the LS_ACC for the FLOGI
wasn't getting intercepted by FIP.

Change to call fcoe_ctlr_els_send when sending any ELS,
not just requests.

Signed-off-by: Joe Eykholt <jeykholt@cisco.com>

---
 drivers/scsi/fcoe/fcoe.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)


---
diff --git a/drivers/scsi/fcoe/fcoe.c b/drivers/scsi/fcoe/fcoe.c
index 2f47ae7..2f3b73c 100644
--- a/drivers/scsi/fcoe/fcoe.c
+++ b/drivers/scsi/fcoe/fcoe.c
@@ -1443,7 +1443,7 @@ int fcoe_xmit(struct fc_lport *lport, struct fc_frame *fp)
 		return 0;
 	}
 
-	if (unlikely(fh->fh_r_ctl == FC_RCTL_ELS_REQ) &&
+	if (unlikely(fh->fh_type == FC_TYPE_ELS) &&
 	    fcoe_ctlr_els_send(&fcoe->ctlr, lport, skb))
 		return 0;
 
