# choose following mode: virtio, dpdk, posix
NETWORK_MODE=posix

# tap device name(virtio)
TAP=tap0

# bridge device name (virtio)
BRIDGE=virbr0

# ethernet device name
IFNAME=eth0

# setup NIC's and disks' interrupts, RPS, XPS, nomerges and I/O scheduler (posix)
SET_NIC_AND_DISKS=no

# ethernet device driver (dpdk)
ETHDRV=

# ethernet device PCI ID (dpdk)
ETHPCIID=

# number of hugepages
NR_HUGEPAGES=64

# user for process (must be root for dpdk)
USER=scylla

# group for process
GROUP=scylla

# scylla home dir
SCYLLA_HOME=/var/lib/scylla

# scylla config dir
SCYLLA_CONF=/etc/scylla

# scylla arguments
SCYLLA_ARGS="--log-to-syslog 0 --log-to-stdout 1 --default-log-level info --network-stack posix"

# setup as AMI instance
AMI=no
